
**6.16-Bit Subtraction for 8085**

****