
**1.8-bit Addition for 8085**

****