3.8-Bit Multiplication for 8085

